|  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- |
| ***S.No*** | ***Particulars*** | ***Unit*** | ***Quantity*** | ***Rate*** | ***Amount*** | ***Remarks*** |
| ***1*** | ***Metallic Work*** |  |  |  |  |  |
|  | Providing and laying of STEEL COLUMN and BEAM where required including all materials, labor, lead and lift as per drawing specification.(3”x3” square pipe along with truss of 2” round pipe) | Ft2 | 2100 |  |  |  |
| ***2*** | ***UPVC Roofing*** |  |  |  |  |  |
|  | Delivery and supply of UPVC roofing on site with fitting including GUTTER and RIDER required and other materials all complete. (Brand: Sunrise Roll top ridge flashings at 3mm floded lengths)  ***UPVC*** | Ft2 | 2576 |  |  |  |
| ***3*** | ***WALL*** |  |  |  |  |  |
|  | Delivery and supply of cement board with fiting and sealing the joints ( Visaka Brand Sandwich panel 50mm thickness, cement based light weight concrete boards.)  ***EXTERNAL WALLS***  ***INERNAL WALLS*** | Ft2  Ft2 | 2300  1050 |  |  |  |
| ***4*** | ***False Ceiling*** |  |  |  |  |  |
|  | Supplying & applying 2”\*3” channel & 12mm Gypsum Board , finished smooth including supply of materials , labor , etc all complete as per drawing , specification & approval of Engineer. | Ft2 | 2240 |  |  |  |
| ***5*** | ***PLANK*** | Ft2 | 270 |  |  |  |
| ***6*** | ***WINDOWS*** |  |  |  |  |  |
|  | Supplying , fabrication & installations of Power Coated Aluminum Window work with 101mm x45mm section, 5mm the, clear glass & all fixing accessories including supply of materials, labor, leveling & all complete as per drawing, specification & approval of engineer. | Ft2 | 350 |  |  |  |
|  | ***Structure Glazing*** | Ft2 | 278.87 |  |  |  |
| ***7*** | ***DOORS*** |  |  |  |  |  |
|  | Supplying 100mm Aluminum series including materials, labor, leveling & all complete as per drawing, specification & approval of engineer. | Ft2 | 110 |  |  |  |
| ***8*** | ***ACP*** | Ft2 | 245 |  |  |  |
|  | | | | |